WATKft

weak
tank

fm>or

?w^^^

PLOO

N2 I

N9    3

*
v////////////////////////////a
qV,

tank

FUOOR

It
£1^
To   "D re, i <
To   Pol-c.her6
fig. 9.—arrangement of bi.hack-mixing plant, using bleaching powder
There are three mixers, fourth wash tank, etc.

TU